 SECTION HEADER
 dc.b 1
 dc.t channel_0

 SECTION CODE
channel_0:
 delay 0
 priority 120
 sfx
 samplerate 4
 volume 0
 patch patch_50
 duration 20
 delay 22
 note sample_02
 duration 24
 delay 26
 note sample_03
 delay 24
 note sample_00
 eos
