 SECTION HEADER
 dc.b 1
 dc.t channel_0

 SECTION CODE
channel_0:
 delay 0
 priority 110
 sfx
 samplerate 4
 patch patch_65
 volume 0
 duration 24
 delay 14
 note sample_15
 delay 24
 note sample_15
 eos
